lb7 and lly's

Fuses to be pulled before flashing:

radio

radio amp

tbc bat

tbc ign

info

Make sure the cig lighter works

All other aftermarket electronics need to be disconnected from power.

aftermarket Radios and harness splicing to factory harness needs to be pulled

Steps, Light bars, Alarm systems, Brake controllers and anything else that did not come factory must be disconnected.

EFI error codes for no communication with control module.

0280, 0281,0101,0537,0333

If you do all of the above and still get one of the above codes, we then need to have a laptop in truck to passthrough flash.